
WEEK-8

USN- 1BM21CS173


DATE-18-08-2023


Create a topology in order to depict TTL of a packet.


TOPOLOGY:



ROUTER CONFIG:











SENDING THE PDU NOTING THE DROP OF TTL VALUE AS IT CROSSES A ROUTER


PC-0 -> PC-1











PC-1 ->PC-0

